Page: 1 of 7

Version: 2.0 Revision Date: 2015/07/01

# SECTION 1： IDENTIFICATION OF THE SUPPLIER AND SUBSTANCE

## MANUFACTURER: ADDRESS:

**Shanghai King Chemical Co,.Ltd**

ROOM CDEF , 9th Floor, Building D, Weijing Center Tower, NO.2337 GuDai Road , Minhang District, Shanghai, China 201199

## Emergency Telephone: Market Service: Technical Service: Fax:

+86-21-67817854

+86-21-67817854

+86-21-67817855

## Identifier used on label: General description: Physical Form:

**Color: Odor: CAS #:**

KC-2206

Acrylic ester copolymer emulsion Liquid

Milky white & bluish Acrylic odor Mixture

|  |
| --- |
| **SECTION 2： HAZARDS IDENTIFICATION** |
| **Classification of the product:** | No need for classification for this product in accordance with **General rule for classification and hazard communication of chemicals (GB13690-2009)** |

|  |
| --- |
| **SECTION 3： COMPOSITION/ INFORMATION ON INGREDIENTS** |
| This product is chemical mixture and does not contain any substances presenting a health or environmental hazard. |
| **CHEMICAL NAME** | **CAS NUMBER** | **CONCENTRATION %** |
| Acrylic ester copolymer | / | 47-49% |
| H2O | 7732-18-5 | 51-53% |
| Polyoxyethylene pentylphenol ether | 9016-45-9 | 1-2% |
| 5-Chloro-2-methyl-3(2H)-isothiazolone | 26172-55-4 | ≤22.5ppm |
| mixt.with2-methyl-3(2H)-isothiazolone | 2682-20-4 | ≤7.5ppm |

Page: 2 of 7

Version: 2.0 Revision Date: 2015/07/01

# SECTION 4： FIRST-AID MEASURES

**Inhalation:**

Move into fresh air.

**Skin contact:**

Wash affected areas thoroughly with soap and water. If skin irritation

persists, seek medical attention.

**Eye contact:**

Rinse with plenty of water for at least 15 minutes. If eye irritation

persists, seek medical attention.

**Ingestion:**

Flush at once and then drink copious amounts of water, seek medical

attention if necessary. Do not give anything by mouth to an unconscious victim.

|  |
| --- |
| **SECTION 5: FIRE-FIGHTING MEASURES** |
| **Suitable media:****Special hazard arising during fire fighting:****Advice for fire-fighters:** | Use extinguishing media appropriate for surrounding fireWhen temperature is above 100℃/212℉, material will splatter and may burn after it is dried.Wear self-contained breathing apparatus and protective clothing |

Page: 3 of 7

Version: 2.0 Revision Date: 2015/07/01

|  |
| --- |
| **SECTION 6: ACCIDENTAL RELEASE MEASURES** |
| **Personal precautions:****Environmental precautions: For small amount:****For large amount: Methods for cleaning up:** | Personal protective equipment should be used. People should be kept away from or upwind of spill/leak. In addition, material may create slippery condition.Do not allow the spills and waste to reach sewage or effluent systems pick up with suitable absorbent material (e.g. sand, soil)Pump off product.Spill should be transfer to suitable container for recovery or disposal. Dispose of material in accordance with local regulations. |

|  |
| --- |
| **SECTION 7: HANDLING AND STORAGE** |
| **Handling：****Storage temperature: Further information:****Other data:** | Avoid contact with eyes. Skin and clothing. Wash thoroughly after handling. Keep container tightly closed. Do not breathe vapor, mist or gas.10℃-35℃Store away from freezing as product stability may be affected. Please stir well before use.Monomer vapors can be evolved when material is heated during processing operations and several types of ventilation are required (see section 8). |

Page: 4 of 7

Version: 2.0 Revision Date: 2015/07/01

# SECTION 8： EXPOSURE CONTROLS/ PERSONAL PROTECTION

## Eye protection:

Safety glasses with side-shields. Eye protection worn must be compatible with respiratory protection system employed.

## Hand protection:

The gloves listed below may provided protection against permeation: Neoprene gloves (Gloves of other chemically resistant materials may not provide adequate protection).

## Respiratory protection:

**Engineering measures:**

Use certified respiratory protection equipment, when respiratory risks cannot be avoided or sufficiently limited by technical means of collective protection or by measures, methods or procedures of work organization.

Use only in area provided with appropriate exhaust ventilation.

|  |
| --- |
| **SECTION 9： PHYSICAL AND CHEMICAL PROPERTIES** |
| **Physical state:** | Liquid | **Color:** | Milky white & bluish |
| **Odor:** | Acylic odor | **PH:** | 8±1 |
| **Boiling point: (water)** | 100℃ | **Flash point:** | Noncombustible |
| **Lower explosion limit:** | Not applicable | **Upper explosion limit:** | Not applicable |
| **Vapor pressure: (water)** | 17mmHg 20℃ | **Relative vapor density:** | <1.00 (water) |
| **Water solubility:** | Dilatable | **Particle Diameter:** | 0.1-0.2μm |
| **Viscosity, dynamic:** | 500-2000cps | **Evaporation rate:** | < 1.00 (water) |
| **Percent volatility:** | 48±1% | **Latex style:** | Anionic |
| **MFFT:** | 28℃ |  |  |
| **Relative density proportion:** | Wet: 1.0-1.1Dry: 1.1-1.2 |  |  |
| **NOTE: The physical data presented above are typical values and should not be construed as a specification.** |

Page: 5 of 7

Version: 2.0 Revision Date: 2015/07/01

## SECTION 10： STABILITY AND REACTIVITY

**Hazardous reactions:**

No hazardous reactions have been reported.

**Materials to avoid:**

There are no known materials that are incompatible with this product.

**Polymerization:**

Product will not undergo polymerization

**Decomposer:**

Acrylic monomer can produced by thermal decomposition

|  |
| --- |
| **SECTION 11： TOXICOLOGICAL INFORMATION** |
| No data are available for this material. This information shown is based on profiles of compositionally similar materials. |
| **Acute oral intoxication:** | half lethal does (LD50)>5,000 mg/kg (rat) |
| **Acute skin toxicity:** | half lethal does (LD50)>5,000 mg/kg (rabbit) |
| **Skin irritation:** | may lead to short-term irritation (rabbit) |
| **Eyes irritation:** | nonirritating (rabbit) |
| **Respiratory intoxication:****Others:** | half lethal does (LD50)>21 mg/l (rat)Polyoxyethylene pentylphenol ether |

|  |
| --- |
| **SECTION 12： ECOLOGICAL INFORMATION** |
| **No data is available for this product.** |

Page: 6 of 7

Version: 2.0 Revision Date: 2015/07/01

|  |
| --- |
| **SECTION 13： DISPOSAL CONSIDERATIONS** |
| **Environmental precautions:** | Keep spills and cleaning waste out of sewage, surface waters or |
|  | effluent systems. |
| **Disposal:** | Coagulate the emulsion by stepwise addition of ferric chloride and |
|  | lime. Remove the clear supernatant and flush to a chemical sewer. For |
|  | disposal, incinerate or landfill at a permitted facility in accordance with |
|  | local regulations. |

|  |
| --- |
| **SECTION 14： TRANSPORT INFORMATION** |
| **Road and Rail transport: Sea transport：****Air transport:****Notice:** | Not regulated (not dangerous for transport) Not regulated (not dangerous for transport) Not regulated (not dangerous for transport)Transportation classifications may vary by container volume and may be influenced by regional or country variations in regulations. |

Page: 7 of 7

Version: 2.0 Revision Date: 2015/07/01

|  |
| --- |
| **SECTION 15： REGULATORY INFORMATION** |
| **General rule for classification and hazard communication of chemicals (GB 13690-2009)****General rules for precautionary label for industrial chemicals (GB 15258-2009)****Inventory of Existing Chemical Substances in China (IECSC)****Toxic Substances Control Act (TSCA)** | Classification has been performed according to regulations.Label has been performed according to regulationAll intentional components are listed on the inventory, are exempt, or are supplier certified.All components of this product are in compliance with the inventory listing requirements of the Toxic Substances Control Act (TSCA) Chemical Substance Inventory. |

|  |
| --- |
| **SECTION 16: OTHER INFORMATION** |
| **Reference:****Notice:** | Safety data sheet for chemical products—Content and order of sections (GB 16483-2008)The information provided in this Safety Data Sheet in accordance with the best of our knowledge, information and belief at the date of its publication. The information given is designed only as guidance for safe handling, use, processing, storage, transportation, disposal and release and is not to be considered a warranty or quality specification. The information relates only to the specific material designated and may not be valid for such material used in combination with any other materials or in any process, unlessspecified in the text. |